Install / Uninstall notes for Sid 20090429 SW release

# Sid 20100401 SW release notes

## Changes

- Major changes were fixing WHQL related issues in preparation for WHQL testing.

ID | Summary
15640 [SEC] | {CTC}:WS-Print: WHQL:WSD-Mon Printer Verification Test fa...
15590 [SEC] | [SID] [KOR,HEB,RUS,FIN,NLD,DAN,CSY,TRK,THA,ROM,IND]KOR-10...
15147 [SEC] | LOC: Device Settings/Basic Control option button label w...
15823 [SEC] | LOC: Device Settings > System Setup - first option name a...
15705 [SEC] | [Loc] [Ell/PTB/FRA/FIN] "Automatically turn off device af...
15591 [SEC] | [Loc] [KOR, NLD] KOR-1lang: Some options of "Size is" Dro...
15575 [SEC] | [Loc] “Status Alerts” is not localized in the device sett...
15746 [SEC] | The job cancelled in the spooler automatically if printin...
15863 [SEC] | The EWS link is seen in the device settings dialog when i...
15831 [SEC] | SM does not exit if cable pulled while alert active
15860 [SEC] | Supplies page does not show OPC info when non-HP OPC note...
15861 [SEC] | Supplies page does not show OPC when life <= 30%
15821 [SEC] | Printing Preferences - Help button no longer opens the he...
15859 [SEC] | Very Low cart missing the *** to connect to note.
15708 [SEC] | [WHQL] PrintDrvStress fails due to error in SD module
15713 [SEC] | [WHQL] Print Gremlin fails with Win32 Exception
15876 [SEC] | "Very" part of "Very Low" translations show up in English...

## Known issues

## Uninstall of previous SW versions

The current SW driver does not have an uninstaller. The uninstall process is as follows:

- Make sure the printer is disconnected or turned off.
- If the Tray Icon is showing in the system tray right click on the icon and select “Hide”. This will cause the tray icon utility to exit so that it can be updated and avoids the need for a second reboot.
- Open the “Printers and Faxes” tool from the control panel.
- Delete all instances of the Sid, CP1025 and CP1025nw printers.
- In the “Printers and Faxes” window click on File->Server Properties.
- Select the Driver tab of the Print Server Properties dialog, highlight the “HP Sid” driver and click the remove button. If notified that the driver cannot be removed because it is in use stop and re-start the spooler by typing “net stop spooler” followed by “net start spooler” on the command line. Then try the remove again.
- Also remove any instances of the CP1025 and CP1025nw printers from the Print Server Properties dialog.
- Remove old instances of the .inf files by:

- Search the .inf directory for oem*.inf files containing 1025. Open and verify that the .inf is indeed a Sid .inf. If it is then delete the .inf and the corresponding .pnf files.

- Reboot (sorry about that).
- Start a command prompt and change into your windows directory and from the windows directory execute the following commands:

- net stop spooler
- del hpcp1020*.* /s
- net start spooler

## Install of current SW version

The current driver must be installed through a Plug and Play install process. It will install only the printer driver.

- Connect the printer to the PC and power it on. Wait for the PnP prompts to start. You will first be prompted to install the LEDM driver followed by the Printer Driver.
- LEDM Install

- When the LEDM PnP Prompt occurs do not allow the installer to search for drivers at Windows Update.
- At the next screen select “Install from a list or specific location”. Click next.
- At the next screen click the Browse button and select the Sid_20091118\bulkiodrv directory.
- Click next and if warned that the SW is not signed click the “Continue Anyway” button.
- Point the installer at the driver directory, select the hppadm14_for_sid.inf. file and continue.
- Once the LEDM PnP install is complete there is a manual step that must be performed before HP’s test application will work. Marvell assumes that this step will be taken care of by the HP installer team in the future. The step is to edit a registry key. Open regedit.exe and locate the following key: HKEY_LOCAL_MACHINE\SYSTEM\CurrentControlSet\Control\DeviceClasses\{211cd2c1-a63e-4164-9e17-fda3fe1f79ff}\##?#USB#Vid_03f0&Pid_0b2a&MI_01#6&2732edb4&0&0001#{211cd2c1-a63e-4164-9e17-fda3fe1f79ff}\#\Device Parameters\Portname

The portion highlighted in orange is created during the install, the part in red might vary from printer to printer – Marvell is not sure what those numbers are referring to. The part in black has to be added manually. The value for Portname can be anything – typically it is the USB port number assigned to your print driver during install. The key is that the value in the registry matches the value used in HP’s test application (this value is configurable).

- Printer Driver Install

- When the PnP prompt for the driver occurs select the “Do not allow it to search Windows Update for software” option.
- At the next screen select “Install from a list or specific location”. Click next.
- At the next screen click the Browse button and select the Sid_20091118 directory.
- Click next and when warned that the SW is not signed click the “Continue Anyway” button.
- If any prompts display asking for a directory point them to the Sid_20091118 directory.
- Once the install is complete click Finish on the final dialog.