| Setup for Mac OS X It is necessary to add the printer driver for your product in the Print Center or Printer Setup Utility menu before printing. Follow the steps below to add the printer driver.

| Note:

- Once you have added the printer driver in the Printer List, you do not need to add it again unless you change printer drivers.

- Ensure you have securely connected the printer to your computer using the interface cable, then turn on the printer.

| Click the Add button in the Print Center or Printer Setup Utility.

| Follow the instructions for your operating system to select the appropriate port and the printer.

For Mac OS X 10.2 to 10.3:
Select the appropriate port referring to the following table for port selection. Then select the printer and click Add in the Printer List dialog.

Connection Type | Selection
USB cable | Select USB
IEEE 1394 cable * IEEE 1394-supported model only | Select EPSON FireWire

For Mac OS X 10.4:
Select the appropriate port and the printer depending on the type of connection you are using.

When using a USB cable to connect the printer, select the printer and then click Add in the Printer Browser dialog.

When using an IEEE 1394 cable (IEEE 1394-supported printers only) to connect the printer, click More Printers in the Printer Browser dialog. Select EPSON FireWire and the printer, then click Add.

| Choose Quit Print Center or Quit Printer Setup Utility from the Print Center or Printer Setup Utility menu.

Top