Other Information

# Specifications

> Supported Image Files

## Supported Image Files

Image formats: | JPEG (JFIF, Exif, CIFF, DCF, EPSON JPEG, Exif2.21DCF2.0) TIFF (Standard non-compressed TIFF files only) BMP (for Windows: excluding images compressed with 16-bit or 32-bit RLE (excluding the Topdown format or the OS2 format).) PICT (for Macintosh, 72 dpi only)

QAD (Windows), QAD2 (Macintosh): (print setting data with EPSON Easy Photo Print)

QLD (Windows), QAD2 (Macintosh): (image processing data produced by EPSON Darkroom Print)

Audio data

Readable image size: | Windows: 573 mega pixels (one side should be 40,000 pixels or less)* Macintosh: 573 mega pixels (one side should be 40,000 pixels or less)*
The maximum readable size is as follows. DSC images: 4,500 x 3,000 pixel Stitching images: 40,000 x 40,000 pixel TWAIN images: 20,400 x 28,080 pixel PICT images: 4,095 x 4,095 pixel

Other images: 4,500 x 3,000 pixel

Note:
The maximum readable size may vary depending on the available hard disk space.

Rotatable image size: | Macintosh: 32,767 pixels or less (the same as the maximum readable image size) less than approximately 13,5 mega pixels.
Save format: | JPEG (quality fixed, JFIF(Ycc) or Exif) (one side should be less than 65,500 pixels) TIFF BMP
Number of image files that can be registered in the My Selection field: | 999 files Note: Providing that the memory and hard disk size is capable of supporting such a number.
DPOF compatible function: | Functions under DPOF version 1.10 are supported.
File formats readable from the digital camera | Windows: Files with the following file extensions (not case-sensitive) .avi, .bmp, .jfif, .jpe, .jpeg, .jpg, .m1v, .mov, .mpg, .mpeg, .qt, .tif, .tiff, .wav Macintosh: Readable if either a file type or file extension is one of the following - Files with the following file types
BMPf, JPEG, MooV, MPEG, PICT, TIFF, VfW, WAVE
- Files with the following file extensions (not case-sensitive)
.avi, .bmp, .jpe, .jpg, .jpeg, .mov, .mpeg, .pct, .pict, .tif, .tiff, .wav

| * Any source can be used to load an image, such as a digital camera, TWAIN source, stitching, and so on.

[Top]