# Index

#

0 slash,

- About Your Printer's Default Settings

Adjusting

> paper-thickness lever,
> - Adjusting the paper-thickness lever

> tear-off position,
> - Adjusting the tear-off position

> top-of-form position,
> - Adjusting the top-of-form position

Aligning vertical lines,

- Printing a Self Test

Auto CR (carriage return),

- About Your Printer's Default Settings

Auto I/F (interface) wait time,

- About Your Printer's Default Settings

Auto line feed,

- About Your Printer's Default Settings

Auto tear-off,

- About Your Printer's Default Settings

Baud rate,

- About Your Printer's Default Settings

Bidirectional (Bi-d) printing.,

- About Your Printer's Default Settings

Built-in font

> list,
> - Mechanical

Buttons.,

- Using the Control Panel

Buzzer (beeper) setting,

- About Your Printer's Default Settings

Character table

> list,
> - Mechanical

> setting,
> - About Your Printer's Default Settings

Cleaning the printer,

- Cleaning the Printer

Contacting EPSON,

- Contacting Customer Support

Continuous paper

> printing,
> - Printing on Continuous Paper

> specifications,
> - For LX-300+
> - For LX-1170

Control panel,

- Using the Control Panel

- Using the Error Indicators

Customer support,

- Contacting Customer Support

Cut-sheet feeder,

- Cut-sheet feeder

Data length,

- About Your Printer's Default Settings

Default settings

> changing,
> - Changing default settings

> option list,
> - About Your Printer's Default Settings

Driver.,

- Using the Printer Driver with Windows Me, 98, and 95

Emulation.,

- IBM 2380 Plus (for LX-300+)/ IBM 2381 Plus (for LX-1170) emulation control codes

Envelopes

> printing,
> - Envelopes

> specifications,
> - For LX-300+
> - For LX-1170

EPSON Remote! utility,

- Using the EPSON Remote! Utility
  (LX-300+ only)

EPSON Status Monitor 3 utility,

- Accessing EPSON Status Monitor 3

Error indication,

- Using the Error Indicators

ESC/P,

- EPSON ESC/P control codes

Font,

- About Your Printer's Default Settings

Font (default setting),

- About Your Printer's Default Settings

High speed draft (default setting),

- About Your Printer's Default Settings

I/F (interface) mode,

- About Your Printer's Default Settings

IBM 2380 Plus/IBM 2381 Plus emulation,

- IBM 2380 Plus (for LX-300+)/ IBM 2381 Plus (for LX-1170) emulation control codes

International character set for Italic table,

- About Your Printer's Default Settings

International character sets,

- Mechanical

Labels

> printing,
> - Labels

> specifications,
> - For LX-300+
> - For LX-1170

Lights.,

- Using the Control Panel

Manual feed wait time,

- About Your Printer's Default Settings

Micro adjust,

- Adjusting the top-of-form position

- Adjusting the tear-off position

Multipart forms

> printing,
> - Multipart forms

> specifications,
> - For LX-300+
> - For LX-300+
> - For LX-1170

Options

> Color upgrade kit,
> - Color upgrade kit (LX-300+ only)

> Cut-sheet feeder,
> - Cut-sheet feeder

> Pull tractor unit,
> - Pull tractor unit

> Roll paper holder,
> - Roll paper holder

Packet mode,

- About Your Printer's Default Settings

Page length for tractor,

- About Your Printer's Default Settings

Panel.,

- Using the Control Panel

Paper alignment,

- Paper alignment

Paper specifications,

- Paper

Paper-thickness lever,

- Adjusting the paper-thickness lever

Parallel I/F (interface) bidirectional mode,

- About Your Printer's Default Settings

Parity,

- About Your Printer's Default Settings

Printable area,

- Printable area

Print direction,

- About Your Printer's Default Settings

Printer driver

> accessing

> > from Windows 2000 or NT 4.0,
> > - Using the Printer Driver with Windows 2000 and NT 4.0

> > from Windows 3.1,
> > - Using the Printer Driver with Windows 3.1

> > from Windows Me, 98 or 95,
> > - Using the Printer Driver with Windows Me, 98, and 95

> > from Windows NT 3.5x,
> > - Using the Printer Driver with Windows NT 3.5x

> settings,
> - Printer Driver Settings Overview

Remote! utility.,

- Using the EPSON Remote! Utility
  (LX-300+ only)

Removing

> printed document from

> > push tractor,
> > - Removing a printed document from the push tractor

Ribbon cartridge,

- Printer Specifications

Roll paper

> default setting,
> - About Your Printer's Default Settings

> printing,
> - Roll paper holder

> specifications,
> - For LX-300+
> - For LX-1170

Roll paper holder,

- Roll paper holder

Safety instructions,

- Important Safety Instructions

Self test,

- Printing a Self Test

Single sheets

> printing,
> - Printing on Single Sheets

> specifications,
> - For LX-300+
> - For LX-1170

Skip over perforation,

- About Your Printer's Default Settings

Software

> default setting,
> - About Your Printer's Default Settings

Specifications

> built-in font,
> - Mechanical

> character tables,
> - Mechanical

> command lists

> > ESC/P,
> > - EPSON ESC/P control codes

> > IBM 2380 Plus/IBM 2381 Plus emulation,
> > - IBM 2380 Plus (for LX-300+)/ IBM 2381 Plus (for LX-1170) emulation control codes

> electrical,
> - Electronic

> environmental,
> - Electrical

> international character sets,
> - Mechanical

> mechanical,
> - Printer Specifications

> paper,
> - Paper

> paper alignment,
> - Paper alignment

> printable area,
> - Printable area

> standards and approvals,
> - Standards and approvals

Status Monitor 3 utility.,

- Accessing EPSON Status Monitor 3

Tear-off,

- Advancing the paper to the tear-off edge

> adjusting,
> - Adjusting the tear-off position

> automatically,
> - Advancing the paper to the tear-off position automatically

> button,
> - Using the Tear Off button

Technical support,

- Contacting Customer Support

Transporting the printer,

- Transporting the Printer

Unidirectional (Uni-d) printing.,

- About Your Printer's Default Settings