Using Bi-D Adjustment

Home > Printer Software

# Using Bi-D Adjustment

Making adjustment with Bi-D Adjustment
This utility tool allows you to make adjustment when you find a misalignment in vertical line.

## Making adjustment with Bi-D Adjustment

To make Bi-D Adjustment, follow the steps below.
Caution:

Do not turn off the printer while the printer is printing adjustment pattern. Doing so may cause the printer to store incorrect settings. If you turned off the printer during the adjustment process, restart Bi-D Adjustment again.
Do not turn off Packet Mode setting.
Network connection is not supported.
Make sure that the printer's status is ready before making Bi-D Adjustment.
This function is only valid when the paper-thickness lever is set to -1, 0, or 1.

| Open the Utility menu, then click the Bi-D Adjustment icon. To find out how to open the Utility menu, see . The Bi-D Adjustment window appears.

| Click Next.

| Click Print. The printer prints three sets of adjustment pattern.

| Look at the adjustment patterns and find the vertical line that is aligned the best. Then, select the corresponding line number in the Bi-D Adjustment window.

| Click Set. The adjustment pattern will be stored in the printer.

Top