Advanced Guide > Printing from a Computer > Printing with Other Application Software > Various Printing Methods > Setting the Stapling Margin

# Setting the Stapling Margin

The procedure for setting the stapling direction and the width of the stapling margin is as follows:

1. Open the printer driver setup window

2. Specify the side to be stapled

   Check the position of the stapling margin from Staple Side on the Page Setup tab.
   The printer analyzes the Orientation and Page Layout settings, and automatically selects the best staple position. If you want to change the setting, select from the list.

3. Set the margin width

   If necessary, click Specify Margin... and set the width of the stapling margin, and then click OK.

4. Complete the setup

   Click OK on the Page Setup tab.
   When you execute print, the data is printed with the specified staple side and margin.

Important

- Staple Side and Specify Margin... appear grayed out and are unavailable when:

  - Poster Printing or Booklet Printing is selected for Page Layout.

  - Scaled Printing is selected for Page Layout (If Duplex Printing is also selected, only Staple Side is selectable).

  - Borderless Printing check box is checked (If Duplex Printing is also selected, only Staple Side is selectable).

Page top