Advanced Guide Troubleshooting

Contents > Appendix > Safety Precautions

# Safety Precautions

Please read the safety warnings and cautions provided in this manual to ensure that you use the printer safely. Do not attempt to use the printer in any way not described in this manual. It causes unexpected accident, fire, or electrical shock.

Warning You may cause an electric shock, fire, or damage the printer if you ignore any of these safety precautions.

> Choosing a location | Do not place the printer close to flammable solvents such as alcohol or thinners.
> Power supply | Never attempt to plug in or unplug the printer from the power supply when your hands are wet.
> Always push the plug all the way into the power outlet.

> Never damage, modify, stretch or excessively bend or twist the power cord. Do not place heavy objects on the power cord.

> Never plug the printer into a power socket that is shared with other equipment (extension lead/cord, 2- or 3-way adapter, etc.).

> Never use the printer if the power cord is bundled or knotted.
> If you detect smoke, unusual smells or strange noises around the printer, immediately unplug the printer at the power supply and call for service.

> Periodically, unplug the printer and use a dry cloth to wipe off any dust or dirt collected on the plug and the power outlet. If the printer is placed at a location exposed to a lot of dust, smoke, or high humidity, the dust collected on the plug absorbs moisture and may cause insulation failure and fire.

> If you hear thunder, disconnect the power supply of the printer and refrain from using it. Leaving the printer plugged in may cause fire, electric shock, or damage to the printer, depending on the thunder storm.
> Use the power cable included with the printer.
> Cleaning the printer |

> Use a damp cloth to clean the printer. Never use flammable solvents such as alcohol, benzene or thinners.

> If flammable solvents come in contact with electrical components inside the printer, it could cause a fire or electric shock.

> Always unplug the printer from the power outlet before cleaning the printer. If you accidentally switch the printer on while cleaning it, you could injure yourself or damage the printer.
> Maintaining the printer | Do not attempt to disassemble or modify the printer. There are no user serviceable parts inside the printer. The printer contains high-voltage components. Never attempt any maintenance procedure not described in this guide.
> Working around the printer | Do not use highly flammable sprays near the printer. This could cause a fire or electric shock if the spray comes into contact with electrical components inside the printer.

Caution You may cause injury or damage the printer if you ignore any of these safety precautions.

> Choosing a location | Do not install the printer in a location that is unstable or subject to excessive vibration.
> Do not install the printer in locations that are very humid or dusty, in direct sunlight, outdoors, or close to a heating source. To avoid the risk of fire or electric shocks, install the printer in a location with an ambient temperature range of 5°C to 35°C (41°F to 95°F) and humidity of 10% to 90% (condensation free).
> Do not place the printer on a thick rug or carpet.
> Do not place the printer with its back attached to the wall.
> Power supply |

> Never remove the plug by pulling on the cord.

> Do not use an extension lead/cord.

> Ensure that the area around the power outlet is kept clear at all times so you can easily unplug the power cord if necessary.

> Working around the printer | Never put your hands or fingers in the printer while it is printing.
> When moving the printer, carry the printer at both ends.
> Do not place any object on the printer.
> Do not place metal objects (paper clips, staples, etc.) or containers of flammable solvents (alcohol, thinners, etc.) on top of the printer.
> If any foreign object (metal or liquid) fall into the printer, unplug the power cord and call for service.
> Do not transport or store the printer on a slant, vertically or upside-down, as the ink may leak and damage the printer.
> FINE Cartridges (Ink Cartridges) | Keep FINE Cartridges (Ink Cartridges) out of the reach of children. In case ink is accidentally licked or swallowed, rinse out mouth or give one or two glasses of water to drink. If irritation or discomfort occurs, obtain medical advice immediately.
> In case ink gets in contact with eyes, rinse with water immediately. In case ink gets in contact with skin, wash with soap and water immediately. If irritation to eyes or skin persists, obtain medical advice immediately.
> Do not shake FINE Cartridges (Ink Cartridges). Ink may spill out and stain clothing or the surrounding area.

> Never touch the electrical contacts or print head nozzles on a FINE Cartridge (Ink Cartridge) after printing.

> The metal parts may be very hot and could cause burns.

> Do not throw FINE Cartridges (Ink Cartridges) into fire.
> Do not attempt to disassemble or modify the FINE Cartridges.
> Do not handle the FINE Cartridges roughly such as applying them excessive pressure or dropping them.

> Do not rinse or wipe the FINE Cartridges.

> Once you have installed the FINE Cartridges, do not remove them unnecessarily.

Note when you place the printer near other electrical appliances such as fluorescent lamps

Place the printer at least 5.91 inches / 15 cm away from other electrical appliances such as fluorescent lamps. If the printer is placed closer to those, it may not be able to work properly due to fluorescent noises.

When you turn off the power

When you turn off the power, always press the Power button and be sure that the Power lamp (in green) has gone out. If you disconnect the power plug from the power outlet when the Power lamp flashes or is lit, the Print Head cannot be protected and you may not be able to print later.

Page top