Advanced Guide > Appendix > Transporting and Storing the Printer

# Transporting and Storing the Printer

When relocating the printer or storing the printer for a long period of time, pack the printer using the original packing materials.

If you do not have the original packing materials, pack the printer carefully using protective material and place it inside a sturdy box.

caution

- Do not transport or store the printer slanted, vertically, or upside-down, as the ink may leak and damage the printer.

1. Turn the printer off.

2. Confirm that the Power lamp is off and unplug the printer.

   important

   - Do not unplug the printer while the Power lamp is lit or flashing green, as it may cause malfunction or damage to the printer, making the printer unable to print.

3. Close the Paper Support.

4. Disconnect the printer cable from the computer and from the printer, and then disconnect the power plug from the printer.

5. Use adhesive tape to secure all the covers on the printer to keep them from opening during transportation. Then pack the printer in the plastic bag.

6. Attach the protective material to the printer when packing the printer.

   important

   - Pack the printer with the FINE Cartridges left installed in the printer.

   note

   - Clearly label the box as "FRAGILE" or "HANDLE WITH CARE".

Page top