Cleaning the Printer

Home > Product Information

# Cleaning the Printer

To keep your printer operating at its best, you should clean it thoroughly several times a year.
Follow these steps to clean your printer:

| Make sure the printer is turned off. Then remove any paper loaded in the printer.

| Remove the paper guide.

| Use a soft brush to carefully brush away all dust and dirt from the outer case and paper guide.

| If the outer case or paper guide is still dirty, clean it with a soft, clean cloth dampened with mild detergent dissolved in water. Keep the printer cover in place and lower the paper guide cover until it lies flat on the top of the printer to prevent water from getting inside the printer.

Caution:

Never use alcohols or thinners to clean the printer; these chemicals can damage the printer components as well as the case. Be careful not to get water on the printer mechanism or electronic components. Do not use a hard or abrasive brush. Do not spray the inside of the printer with lubricants; unsuitable lubricants can damage the printer mechanism. Contact an EPSON dealer if you think lubrication is needed.