Advanced Guide > Troubleshooting > FINE Cartridge Holder Does Not Move to the Position for Replacing

# FINE Cartridge Holder Does Not Move to the Position for Replacing

- Check 1: Is the Power lamp off?

  Check if the Power lamp is lit green.

  The FINE Cartridge Holder will not move unless the power is on. If the Power lamp is off, close the Front Cover and turn the printer on.

  While the Power lamp is flashing green, the printer is initializing. Wait until the Power lamp stops flashing and remains lit green, and then open the Front Cover again.

- Check 2: Is the Alarm lamp flashing?

  Close the Front Cover, confirm the number of times the Alarm lamp is flashing, take the appropriate action to resolve the error, and then reopen it. For details on how to resolve the error, see Alarm Lamp Flashes Orange.

- Check 3: Has the Front Cover been left open for 10 minutes or longer?

  If the Front Cover is left open for more than 10 minutes, the FINE Cartridge Holder moves to the right to prevent the Print Head from drying out. Close and reopen the Front Cover to return the FINE Cartridge Holder to the left.

- Check 4: Has the printer been printing continuously for a long period?

  Close the Front Cover, wait a while, then reopen it.

  If the printer has been printing continuously for a long time, the Print Head will overheat, and the printer stops printing temporarily to protect the Print Head.

note

- Opening the Front Cover while printing moves the FINE Cartridge Holder to the right. Close the Front Cover, and reopen it after printing is complete.

Page top